**New Juniper device setting**

Connect console cable to the “con port” on the back of the device.

Enter root

At” %”, input “cli” enter “>”

At” >”, input “configure”

Enter “#”

Set the root password in order to initialize.

#set system root-authentication plain-text-password

(For future maintenance, recommended password is “abc123”)